# :LTESt:MEASure:MLIMit:FREGion

:LTESt Measurement Setup Commands

- :LTESt:MEASure:MLIMit:CFMargin
- :LTESt:MEASure:MLIMit:CFResults
- :LTESt:MEASure:MLIMit:FREGion
- :LTESt:MEASure:MLIMit:LLIMit
- :LTESt:MEASure:MLIMit:SOFailure
- :LTESt:MEASure:MLIMit:SOURce:LOCation
- :LTESt:MEASure:MLIMit:SOURce:TYPE
- :LTESt:MEASure:MLIMit:STATe
- :LTESt:MEASure:MLIMit:ULIMit
- :LTESt:MEASure:MLIMit:UPACtion

## Command Syntax

    :LTESt:MEASure:MLIMitN:FREGion {INSide | OUTSide}

Where N identifies one of sixteen {1:16} limit tests.

## Query Syntax

    :LTESt:MEASure:MLIMitN:FREGion?

## Description

Defines when to fail a measurement limit test. Use one of the following arguments:

INSide
  A measurement is counted as a failure if it is within the lower and upper limits, which are set by the `:LTESt:MEASure:MLIMit:LLIMit` and `:LTESt:MEASure:MLIMit:ULIMit` sibling commands.
OUTSide
  A measurement is counted as a failure when the measurement results exceed the parameters set by `:LTESt:MEASure:MLIMit:LLIMit` and `:LTESt:MEASure:MLIMit:ULIMit` sibling commands

Use the `:LTESt:MEASure:MLIMit:STATe` sibling command to start the limit test.

## Example

    :LTESt:MEASure:MLIMit2:FREGion INSide  //  Limit test 2 fails for inside violations.