# :TRIGger:SHOLd:CSOurce:EDGE

:TRIGger Setup And Hold Commands

- :TRIGger:SHOLd:DSOurce
- :TRIGger:SHOLd:CSOurce:EDGE
- :TRIGger:SHOLd:CSOurce
- :TRIGger:SHOLd:HTIMe
- :TRIGger:SHOLd:MODE
- :TRIGger:SHOLd:STIMe

## Command Syntax

    :TRIGger:SHOLd:CSOurce:EDGE  {POSitive | NEGative}

## Query Syntax

    :TRIGger:SHOLd:CSOurce:EDGE?

## Description

In the Setup And Hold trigger mode (see `:TRIGger:MODE`), this command specifies the edge of the Clock Source (see `:TRIGger:SHOLd:DSOurce`) that will trigger.