# :FUNCtion:PARameters:GATing:REGion

Gating Parameters Commands

- :FUNCtion:PARameters:GATing:REGion

## Command Syntax

    :FUNCtionN:PARameters:GATing:REGion {REGion{1:8}}

Where N identifies one of up to 64 possible operators {1:64} that can be defined as part of a math function. The operators are numbered in the order that they were originally added to the function.

## Query Syntax

    :FUNCtionN:PARameters:GATing:REGion?

## Description

Selects the region used to delimit the gating function (`:FUNCtion:FOPerator`). This region must be defined for the same waveform source that is the input to the function.

## Example Command Sequence

    :FUNCtion2:FOPerator GATing
    :FUNCtion2:PARameters:GATing:REGion REGion1
    :FUNCtion2:COLor TCOLor4
    :FUNCtion2:DISPlay ON
    *OPC?
    …
                      //  Your code to synchronize execution timing.