# :ACQuire:COUNt

:ACQuire Commands

- :ACQuire Subsystem
- :ACQuire:CDISplay
- :ACQuire:COUNt
- :ACQuire:POINts
- :ACQuire:POINts:AUTO
- :ACQuire:RUN
- :ACQuire:SINGle
- :ACQuire:SMODe
- :ACQuire:SRATe
- :ACQuire:SRATe:AUTO
- :ACQuire:STATe?
- :ACQuire:STOP

## Command Syntax

    :ACQuire:COUNt <count>

<count> is an int.

## Query Syntax

    :ACQuire:COUNt?

## Description

When the AVERage acquisition sampling mode is selected (see `:ACQuire:SMODe`), this command specifies the number of waveforms/acquisitions to average to give the averaged waveform result. You can enter a value between 2 and 1M. The default value for the number of averages is 16.

## Common Numerical Child Commands

This command supports the use of the following common numerical child commands: `:DEFault`, `:MAXimum`, `:MINimum`, and `:STEP`.