# :MEASure:JITTer:NOISe:ANALysis

Noise Setup Commands

- :MEASure:JITTer:NOISe:ANALysis
- :MEASure:JITTer:NOISe:ERNValue:LEVel
- :MEASure:JITTer:NOISe:MLOCation
- :MEASure:JITTer:NOISe:RNBandwidth
- :MEASure:JITTer:NOISe:RNComp
- :MEASure:JITTer:NOISe:RNCValue:LEVel
- :MEASure:JITTer:NOISe:RNSTabilize
- :MEASure:JITTer:NOISe:RNSValue:LEVel
- :MEASure:JITTer:NOISe:UNITs

## Command Syntax

    :MEASure:JITTerN:NOISe:ANALysis {ON | OFF | 1 | 0}

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Syntax

    :MEASure:JITTerN:NOISe:ANALysis?

## Query Response

    {1 | 0}

## Description

Enables or disables the Noise analysis.