# :CHANnel:COPY

:CHANnel General Commands

- :CHANnel:ATTenuation?
- :CHANnel:COLor
- :CHANnel:COPY
- :CHANnel:COUPling
- :CHANnel:CWINdow
- :CHANnel:DB?
- :CHANnel:DISPlay
- :CHANnel:IMPedance
- :CHANnel:GAIN?
- :CHANnel:PATTern:FILE:GCODe
- :CHANnel:PATTern:FILE:NAME
- :CHANnel:PATTern:FILE:RELoad
- :CHANnel:PATTern:INVert
- :CHANnel:PATTern:KPATtern
- :CHANnel:PATTern:MODE
- :CHANnel:SIGNal:TYPE
- :CHANnel:SKEW
- :CHANnel:SNOise:CALibrate
- :CHANnel:SNOise:SNValue:LEVel{0:3}?
- :CHANnel:SRANge?
- :CHANnel:STATus?
- :CHANnel:UNAMe

## Command Syntax

    :CHANnelN:COPY {CHANnel
                        <source>
                    }

Where N identifies a destination channel into which settings are copied. N is in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, `CHANnel1_2`.

Where <source> identifies a source channel from which to copy settings. <source> is in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, `2B`.

## Description

Copies channels settings from a source channel into the destination channel. Copied settings include the following:

- Scale
- Offset
- Hardware Skew
- Software Delay
- Signal Type Auto Detect and Type
- External Transducer settings
- External Attenuator settings

The copied settings do not include waveform color or any custom waveform name.