# :NETWorks:TRACe:THReshold:GENeral:HYSTeresis

:NETWorks:TRACe Threshold Commands

- :NETWorks:TRACe:TBASe:GENeral:METHod
- :NETWorks:TRACe:TBASe:RFALl:METHod
- :NETWorks:TRACe:THReshold:GENeral:AUTO
- :NETWorks:TRACe:THReshold:GENeral:BASE
- :NETWorks:TRACe:THReshold:GENeral:HYSTeresis
- :NETWorks:TRACe:THReshold:GENeral:LOWer
- :NETWorks:TRACe:THReshold:GENeral:METHod
- :NETWorks:TRACe:THReshold:GENeral:MIDDle
- :NETWorks:TRACe:THReshold:GENeral:PLOWer
- :NETWorks:TRACe:THReshold:GENeral:PMIDdle
- :NETWorks:TRACe:THReshold:GENeral:PUPPer
- :NETWorks:TRACe:THReshold:GENeral:STZero
- :NETWorks:TRACe:THReshold:GENeral:TOP
- :NETWorks:TRACe:THReshold:GENeral:TRACking
- :NETWorks:TRACe:THReshold:GENeral:UPPer
- :NETWorks:TRACe:THReshold:RFALl:BASE
- :NETWorks:TRACe:THReshold:RFALl:LOWer
- :NETWorks:TRACe:THReshold:RFALl:METHod
- :NETWorks:TRACe:THReshold:RFALl:PLOWer
- :NETWorks:TRACe:THReshold:RFALl:PUPPer
- :NETWorks:TRACe:THReshold:RFALl:TOP
- :NETWorks:TRACe:THReshold:RFALl:TRACking
- :NETWorks:TRACe:THReshold:RFALl:UPPer

## Command Syntax

    :NETWorks:TRACeN:THReshold:GENeral:HYSTeresis <plus_or_minus_value>

<plus_or_minus_value> is a double.

Where N identifies a specific trace and must be selected from 1 to 128 {1:128}.

## Query Syntax

    :NETWorks:TRACeN:THReshold:GENeral:HYSTeresis?

## Description

When the `:NETWorks:TRACe:THReshold:GENeral:METHod` setting is `HYSTeresis`, this command sets the user-defined ±hysteresis value for the waveform source.

Use the `:NETWorks:TRACe:THReshold:GENeral:MIDDle` command to enter the center threshold level.