# :LTESt:MTESt:MRESult{N}:CTYPe

:LTESt Mask Limit Commands

- :LTESt:MTESt:MRESult{N}:CTYPe
- :LTESt:MTESt:MRESult{N}:CTYPe:UINTervals
- :LTESt:MTESt:MRESult{N}:CTYPe:WAVeforms
- :LTESt:MTESt:MRESult{N}:SOFailure
- :LTESt:MTESt:MRESult{N}:STATe
- :LTESt:MTESt:SIMage:FNAMe
- :LTESt:MTESt:SIMage:FNAMe:AUPDate
- :LTESt:MTESt:SIMage:FNAMe:USTandard
- :LTESt:MTESt:SIMage:FTYPe?
- :LTESt:MTESt:SIMage:IMETadata
- :LTESt:MTESt:SIMage:INVert
- :LTESt:MTESt:SIMage:MONochrome
- :LTESt:MTESt:SIMage:SINClude
- :LTESt:MTESt:SIMage:STATe
- :LTESt:MTESt:SIMage:WINDow
- :LTESt:MTESt:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:MTESt:SWAVeform:CHANnel:FTYPe
- :LTESt:MTESt:SWAVeform:CHANnel{N}:STATe
- :LTESt:MTESt:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:MTESt:SWAVeform:CMODe{N}:FNAMe
- :LTESt:MTESt:SWAVeform:CMODe:FTYPe
- :LTESt:MTESt:SWAVeform:CMODe{N}:STATe
- :LTESt:MTESt:SWAVeform:CMODe{N}:WMEMory
- :LTESt:MTESt:SWAVeform:DIFF{N}:FNAMe
- :LTESt:MTESt:SWAVeform:DIFF:FTYPe
- :LTESt:MTESt:SWAVeform:DIFF{N}:STATe
- :LTESt:MTESt:SWAVeform:DIFF{N}:WMEMory
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:STATe
- :LTESt:MTESt:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:MTESt:SWAVeform:RESet

## Command Syntax

    :LTESt:MTESt:MRESult{1:16}:CTYPe  {FORever | WAVeforms | UINTervals}

Where {1:16} identifies the specific mask for which to apply the limit test.

## Query Syntax

    :LTESt:MTESt:MRESult{1:16}:CTYPe?

## Query Response

    {FOR | WAV | UINT}

## Description

This command selects the mask Limit Test 'Run Until' Condition:

FORever
  The limit test runs forever.
WAVeforms
  The limit test runs until a number of waveforms are tested. Use the `:LTESt:MTESt:MRESult{N}:CTYPe:WAVeforms` command to specify the number of waveforms.
UINTervals
  The limit test runs until a number of Unit Intervals (UIs) are tested. Use the `:LTESt:MTESt:MRESult{N}:CTYPe:UINTervals` command to specify the number of Unit Intervals.