# :WMEMory:LOAD:SOURce

:WMEMory Loading Commands

- :WMEMory:LOAD
- :WMEMory:LOAD:SOURce
- :WMEMory:FILE:LOAD
- :WMEMory:FILE:NAME

## Command Syntax

    :WMEMoryN:LOAD:SOURce <source_waveform>

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

Where <source_waveform> can be one of the following:

- `CHANnel<connection1-8>_<ch1-8>`; With connection 1, the "`1_`" part is optional, and you can simply use `CHANnel<ch1-8>`.
- `DIFF{1:4}`
- `CGMemory{1:8}`
- `FUNCtion{1:64}`

## Query Syntax

    :WMEMoryN:LOAD:SOURce?

## Description

Selects the source waveform to load into waveform memory. Use the `:CGMemory:LOAD` command to actually load the selected source.

## Example Command Sequence

    :WMEMory2:LOAD:SOURce CHAN3
    :WMEMory2:LOAD

## Parent Command

- `:WMEMory:LOAD`