# :LTESt:LLINe:SWAVeform:DIFF{N}:WMEMory

:LTESt Limit Line Commands

- :LTESt:LLINe:TEST{N}:MODE
- :LTESt:LLINe:TEST{N}:STATe
- :LTESt:LLINe:SIMage:FNAMe
- :LTESt:LLINe:SIMage:FNAMe:AUPDate
- :LTESt:LLINe:SIMage:FNAMe:USTandard
- :LTESt:LLINe:SIMage:FTYPe?
- :LTESt:LLINe:SIMage:IMETadata
- :LTESt:LLINe:SIMage:INVert
- :LTESt:LLINe:SIMage:MONochrome
- :LTESt:LLINe:SIMage:SAVE
- :LTESt:LLINe:SIMage:SINClude
- :LTESt:LLINe:SIMage:STATe
- :LTESt:LLINe:SIMage:WINDow
- :LTESt:LLINe:SSUMmary:FNAMe
- :LTESt:LLINe:SSUMmary:STATe
- :LTESt:LLINe:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:LLINe:SWAVeform:CHANnel:FTYPe
- :LTESt:LLINe:SWAVeform:CHANnel{N}:STATe
- :LTESt:LLINe:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:LLINe:SWAVeform:CMODe{N}:FNAMe
- :LTESt:LLINe:SWAVeform:CMODe:FTYPe
- :LTESt:LLINe:SWAVeform:CMODe{N}:STATe
- :LTESt:LLINe:SWAVeform:CMODe{N}:WMEMory
- :LTESt:LLINe:SWAVeform:DIFF{N}:FNAMe
- :LTESt:LLINe:SWAVeform:DIFF:FTYPe
- :LTESt:LLINe:SWAVeform:DIFF{N}:STATe
- :LTESt:LLINe:SWAVeform:DIFF{N}:WMEMory
- :LTESt:LLINe:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:LLINe:SWAVeform:FUNCtion{N}:STATe
- :LTESt:LLINe:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:LLINe:SWAVeform:RESet

## Command Syntax

    :LTESt:LLINe:SWAVeform:DIFF{N}:WMEMory WMEMory{1:8}

{N} identifies the differential waveform, which must be selected from "<connection1-8>_<ch1,3,5,7>". For example, the differential waveform of connection 4 channels 1 and 2 would be identified as DIFF4_1.

## Query Syntax

    :LTESt:LLINe:SWAVeform:DIFF{N}:WMEMory?

## Description

Upon completion of limit testing for a limit line test, any differential waveform can be automatically saved to one of eight available waveform memory locations. Use this command to associate a specific waveform memory to a specific differential waveform. To actually enable differential waveforms to be saved, use the `:LTESt:LLINe:SWAVeform:DIFF{N}:STATe` command.

To enable limit testing for a limit line test, use the `:LTESt:LLINe:TEST{N}:STATe` command.