# Message 11

## Message

"11. setting is set to limit: Entry was out of range"

## Description

This is a general message that indicates that the specified control or setting was set to its limit. This can be the result of a front-panel change or a remote command that has an argument that is beyond the range of acceptable values. For example, when defining a CTLE math signal processing function you can define a 2 or 3 pole operator. If a 4 pole operator is specified, this error message will be reported.

This message is displayed in the message area and is reported as a programming error message.