# :MEASure:EYE:USER:USER{N}:STATus?

User-Defined Eye Measurement Commands

- :MEASure:EYE:USER:USER{N}
- :MEASure:EYE:USER:USER{N}:ABBReviation?
- :MEASure:EYE:USER:USER{N}:CFILe
- :MEASure:EYE:USER:USER{N}:CFILe:CLEar
- :MEASure:EYE:USER:USER{N}:CFILe:RELoad
- :MEASure:EYE:USER:USER{N}:CFLoaded?
- :MEASure:EYE:USER:USER{N}:COMMents?
- :MEASure:EYE:USER:USER{N}:FAVorite
- :MEASure:EYE:USER:USER{N}:LOCation?
- :MEASure:EYE:USER:USER{N}:LSTatus?
- :MEASure:EYE:USER:USER{N}:LSTatus:REASon?
- :MEASure:EYE:USER:USER{N}:NAME?
- :MEASure:EYE:USER:USER{N}:SOURce{1:2}
- :MEASure:EYE:USER:USER{N}:STATus?
- :MEASure:EYE:USER:USER{N}:STATus:DETails?
- :MEASure:EYE:USER:USER{N}:STATus:REASon?

## Query Syntax

    :MEASure:EYE:USER:USER{1:8}:STATus?

## Query Response

    {CORR | INV | QUES}

CORR
  The measurement result is correct.
INV
  The measurement result is invalid. A question mark (?) is shown in the displayed results table instead of a measurement result.
QUES
  The measurement result is questionable. A question mark (?) is shown in the displayed results table next to the measurement result.

## Description

Queries the status of the `:MEASure:EYE:USER:USER{N}` measurement. Use the `:MEASure:EYE:USER:USER{N}:STATus:REASon?` child query to determine the reason for an invalid or questionable measurement. Additional information about the failure may be available using the `:MEASure:EYE:USER:USER{N}:STATus:DETails?` child query.

## See Also

- Measurement Errors