# :MEASure:EYE:PAM:VECLosure:EYE

PAM Vert. Eye Closure Commands

- :MEASure:EYE:PAM:VECLosure
- :MEASure:EYE:PAM:VECLosure:DEFine:EOPening
- :MEASure:EYE:PAM:VECLosure:DEFine:EOPening:PROBability
- :MEASure:EYE:PAM:VECLosure:EYE
- :MEASure:EYE:PAM:VECLosure:FAVorite
- :MEASure:EYE:PAM:VECLosure:LOCation?
- :MEASure:EYE:PAM:VECLosure:SOURce
- :MEASure:EYE:PAM:VECLosure:STATus?
- :MEASure:EYE:PAM:VECLosure:STATus:DETails?
- :MEASure:EYE:PAM:VECLosure:STATus:REASon?

## Command Syntax

    :MEASure:EYE:PAM:VECLosure:EYE {EYE0}

## Query Syntax

    :MEASure:EYE:PAM:VECLosure:EYE?

## Query Response

     {EYE0}

## Description

This command allows you to select an eye on PAM signals. For NRZ signals, the 0 eye is automatically selected and cannot be changed. The command selects the PAM eye on which to perform the `:MEASure:EYE:PAM:VECLosure`. The query form of the command returns the currently selected eye.

NRZ Waveform
PAM3 Waveform
PAM4 Waveform