# Jitter Measurement Commands

Jitter

- Jitter Setup
- Jitter Measurement Commands
- Jitter Graph Commands
- Noise Setup
- Noise Measurement Commands
- Noise Graph Commands
- Jitter/Noise Advanced Setup

The Jitter analysis measurement commands include:

- :MEASure:JITTer:JITTer:DCD? — DCD, Duty Cycle Distortion
- :MEASure:JITTer:JITTer:DDJ? — DDJ (p-p), Data Dependent Jitter
- :MEASure:JITTer:JITTer:DDPWs? — DDPWS, Data Dependent Pulse Width Shrinkage
- :MEASure:JITTer:JITTer:DJ? — DJ (δ-δ), Deterministic Jitter
- :MEASure:JITTer:JITTer:EWIDth? — Eye Width
- :MEASure:JITTer:JITTer:FOVer2? — F/2 (pk), Even/Odd Jitter
- :MEASure:JITTer:JITTer:ISI? — ISI-J (p-p), Inter-Symbol Interference
- :MEASure:JITTer:JITTer:PJ? — PJ (δ-δ), Periodic Jitter Delta-Delta
- :MEASure:JITTer:JITTer:PJRMs? — PJ (rms), Periodic Jitter RMS
- :MEASure:JITTer:JITTer:RJ? — RJ (rms), Random Jitter RMS
- :MEASure:JITTer:JITTer:TJ? — TJ (p-p), Total Jitter
- :MEASure:JITTer:JITTer:TRANsitions? — # transitions contributing to measurements
- :MEASure:JITTer:JITTer:UDJDd? — UDJ (δ-δ), Uncorrelated Deterministic Jitter
- :MEASure:JITTer:JITTer:UTJ? — UTJ (p-p), Uncorrelated Total Jitter