# :MEASure:FFT:FFRequency:FPLevel

FFT Frequency Commands

- :MEASure:FFT:FFRequency
- :MEASure:FFT:FFRequency:FAVorite
- :MEASure:FFT:FFRequency:FPLevel
- :MEASure:FFT:FFRequency:FPNumber
- :MEASure:FFT:FFRequency:LOCation?
- :MEASure:FFT:FFRequency:SOURce
- :MEASure:FFT:FFRequency:STATus?
- :MEASure:FFT:FFRequency:STATus:DETails?
- :MEASure:FFT:FFRequency:STATus:REASon?

## Command Syntax

    :MEASure:FFT:FFRequency:FPLevel <dBm>

<dBm> is a double.

## Query Syntax

    :MEASure:FFT:FFRequency:FPLevel?

## Description

Defines the threshold an FFT peak must cross to be considered a peak in the FFT Frequency measurement (`:MEASure:FFT:FFRequency`). The default Peak Level is -40 dBm.