# :CALibrate:CONNection:TIMebase:EXPort

:CALibrate Connection Commands

- :CALibrate:CONNection:CLOCk
- :CALibrate:CONNection:ENABled
- :CALibrate:CONNection:EXPort
- :CALibrate:CONNection:IMPort
- :CALibrate:CONNection:SKEW:ENABled
- :CALibrate:CONNection:SKEW:STATus?
- :CALibrate:CONNection:SKEW:STATus:DETails?
- :CALibrate:CONNection:SKEW:STATus:DTEMperature?
- :CALibrate:CONNection:SKEW:STATus:TIME?
- :CALibrate:CONNection:STARt
- :CALibrate:CONNection:STATus?
- :CALibrate:CONNection:STATus:DETails?
- :CALibrate:CONNection:STATus:DTEMperature?
- :CALibrate:CONNection:STATus:TIME?
- :CALibrate:CONNection:TIMebase:ENABled
- :CALibrate:CONNection:TIMebase:EXPort
- :CALibrate:CONNection:TIMebase:IMPort
- :CALibrate:CONNection:TIMebase:STARt
- :CALibrate:CONNection:TRIGger:ENABled
- :CALibrate:CONNection:VERTical
- :CALibrate:CONNection:VERTical:STATus?
- :CALibrate:CONNection:VERTical:STATus:DETails?
- :CALibrate:CONNection:VERTical:STATus:DTEMperature?
- :CALibrate:CONNection:VERTical:STATus:TIME?

## Command Syntax

    :CALibrate:CONNectionN:TIMebase:EXPort "filename"

Where N identifies a specific instrument by connection number and must be selected from {1:8}.

## Description

This command exports to a file the Timebase Adjustment factors for the instrument at the specified connection.