# :MEASure:JITTer:NOISe:GRAPh:TIHist

Noise Graph Commands

- :MEASure:JITTer:NOISe:GRAPh:ABAThtub
- :MEASure:JITTer:NOISe:GRAPh:CTIHist
- :MEASure:JITTer:NOISe:GRAPh:IFILter
- :MEASure:JITTer:NOISe:GRAPh:ISIHist
- :MEASure:JITTer:NOISe:GRAPh:ISISymbol
- :MEASure:JITTer:NOISe:GRAPh:NSPectrum
- :MEASure:JITTer:NOISe:GRAPh:RNPihist
- :MEASure:JITTer:NOISe:GRAPh:RPSPectrum
- :MEASure:JITTer:NOISe:GRAPh:TIHist
- :MEASure:JITTer:NOISe:GSIZe
- :MEASure:JITTer:NOISe:MGRaph
- :MEASure:JITTer:NOISe:NDBValue

## Command Syntax

    :MEASure:JITTerN:NOISe:GRAPh:TIHist {ON | OFF | 1 | 0}

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Syntax

    :MEASure:JITTerN:NOISe:GRAPh:TIHist?

## Query Response

    {1 | 0}

## Description

Enables or disables the TI Histogram jitter graph.