# :CALibrate:CHANnel:STATus:TIME?

:CALibrate Channel Commands

- :CALibrate:CHANnel:ENABled
- :CALibrate:CHANnel:NOISe?
- :CALibrate:CHANnel:STATus?
- :CALibrate:CHANnel:STATus:DETails?
- :CALibrate:CHANnel:STATus:DTEMperature?
- :CALibrate:CHANnel:STATus:TIME?

## Query Syntax

    :CALibrate:CHANnelN:STATus:TIME?

Where N identifies a specific channel in the form "<connection1-8>_<ch1-8>". With connection 1, the connection number part (that is, "1_") is optional, and you can simply use the channel number "<ch1-8>". For example, connection 4 channel 2 is `CHANnel4_2`.

## Description

Queries the date and time when the last channel calibration was performed. If a calibration has not yet been performed, an empty string is returned.

## Example Returned Status String

    "09/20/2012 15:11:05"

## Parent Command

- `:CALibrate:CHANnel:STATus?`