# :MEASure:JITTer:JITTer:RJCResult?

Jitter Setup Commands

- :MEASure:JITTer:BSCale
- :MEASure:JITTer:GSCale
- :MEASure:JITTer:JITTer:ANALysis
- :MEASure:JITTer:JITTer:DIMensions
- :MEASure:JITTer:JITTer:DMAXimized
- :MEASure:JITTer:JITTer:EDGE
- :MEASure:JITTer:JITTer:EOPening
- :MEASure:JITTer:JITTer:EOPening:PROBability
- :MEASure:JITTer:JITTer:FLAG
- :MEASure:JITTer:JITTer:FLEad
- :MEASure:JITTer:JITTer:MODE
- :MEASure:JITTer:JITTer:NUINtervals
- :MEASure:JITTer:JITTer:PTYPe
- :MEASure:JITTer:JITTer:RJBandwidth
- :MEASure:JITTer:JITTer:RJComp
- :MEASure:JITTer:JITTer:RJCResult?
- :MEASure:JITTer:JITTer:RJCValue
- :MEASure:JITTer:JITTer:RJSTabilize
- :MEASure:JITTer:JITTer:RJSValue
- :MEASure:JITTer:JITTer:SMEThod
- :MEASure:JITTer:JITTer:TJBer
- :MEASure:JITTer:JITTer:UNITs
- :MEASure:JITTer:SOURce

## Query Syntax

    :MEASure:JITTerN:JITTer:RJCResult?

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Query Response

<RJ_compensation_result> is a double value.

## Description

This query returns the RJ compensation result.

When using custom RJ compensation (see `:MEASure:JITTer:JITTer:RJComp`), this query returns the custom RJ compensation value and is equivalent to the `:MEASure:JITTer:JITTer:RJCValue` query.

When using automatic RJ compensation values derived from the RN compensation (see `:MEASure:JITTer:JITTer:RJComp`), this query returns a value that is calculated from slew rate and noise. (RN compensation is specified by the `:MEASure:JITTer:NOISe:RNComp` command.)

When RJ compensation is off (see `:MEASure:JITTer:JITTer:RJComp`), this query returns zero.