# :LTESt:ACQuire:SIMage:MONochrome

:LTESt Acquisition Commands

- :LTESt:ACQuire:CTYPe
- :LTESt:ACQuire:CTYPe:SAMPles
- :LTESt:ACQuire:CTYPe:WAVeforms
- :LTESt:ACQuire:SIMage:FNAMe
- :LTESt:ACQuire:SIMage:FNAMe:AUPDate
- :LTESt:ACQuire:SIMage:FNAMe:USTandard
- :LTESt:ACQuire:SIMage:FTYPe?
- :LTESt:ACQuire:SIMage:IMETadata
- :LTESt:ACQuire:SIMage:INVert
- :LTESt:ACQuire:SIMage:MONochrome
- :LTESt:ACQuire:SIMage:SINClude
- :LTESt:ACQuire:SIMage:STATe
- :LTESt:ACQuire:SIMage:WINDow
- :LTESt:ACQuire:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CHANnel:FTYPe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:CMODe{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CMODe:FTYPe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:STATe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:WMEMory WMEMory{1:8}
- :LTESt:ACQuire:SWAVeform:DIFF{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:DIFF:FTYPe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:STATe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:STATe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:RESet

## Command Syntax

    :LTESt:ACQuire:SIMage:MONochrome {ON | OFF | 1 | 0}

## Query Syntax

    :LTESt:ACQuire:SIMage:MONochrome?

## Query Response

    {1 | 0}

## Description

Turns monochrome screen capture on and off when reporting a screen capture for an acquisition limit test. When on, a black and white image will be captured and saved into a file by the `:LTESt:ACQuire:SIMage:FNAMe` command. Selecting monochrome automatically inverts the graticule area's background color. Use the `:LTESt:ACQuire:SIMage:STATe` command to enable screen captures to be saved when the limit test completes. To enable or disable acquisition limit tests, use the `:LTESt:ACQuire:STATe` command.