# Instrument Configuration

Subtopics

- Virtual (Simulated) 4/8 Channel Oscilloscopes

To configure instrument connections:

1. Click the "+" ("Turn Signals On or Off...") button, located in the badges bar, between the Waveform badges and the Horizontal badge.

2. In the Signal Management dialog box, click the associated "+" add button associated with Analog Channels.

3. In the Instrument Configuration dialog box, drag an instrument from the Instruments palette at the top of the dialog box into a Connection at the bottom of the dialog box.

   Infiniium 2026 supports up to eight instrument connections.

4. Now, you can typically click the instrument icon or buttons to connect to, or further set up, the instrument.

A total of 64 input channels are possible. The Infiniium 2026 software can simultaneously display and perform measurements on all 64 channels.

For more information on configuring instruments, see:

- Virtual (Simulated) 4/8 Channel Oscilloscopes