# :MEASure:DATA:UINTerval:STATus:DETails?

Unit Interval Commands

- :MEASure:DATA:UINTerval
- :MEASure:DATA:UINTerval:DWMode
- :MEASure:DATA:UINTerval:FAVorite
- :MEASure:DATA:UINTerval:LOCation?
- :MEASure:DATA:UINTerval:NDRate
- :MEASure:DATA:UINTerval:OCCurrences
- :MEASure:DATA:UINTerval:REGion
- :MEASure:DATA:UINTerval:SOURce
- :MEASure:DATA:UINTerval:STATus?
- :MEASure:DATA:UINTerval:STATus:DETails?
- :MEASure:DATA:UINTerval:STATus:REASon?
- :MEASure:DATA:UINTerval:UREFerence:STATe
- :MEASure:DATA:UINTerval:UREFerence:VALue

## Query Syntax

    :MEASure:DATA:UINTerval:STATus:DETails?

## Description

Returns a string that may provide additional details for a failed `:MEASure:DATA:UINTerval` measurement. If the measurement was successful, a null string is returned.

For a basic description of a measurement failure, use the `:MEASure:DATA:UINTerval:STATus:REASon?` sibling query. Use the `:MEASure:DATA:UINTerval:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors