# :MEASure:HORizontal:DTIMe:STATus:DETails?

Delta Time Commands

- :MEASure:HORizontal:DTIMe
- :MEASure:HORizontal:DTIMe:EDIRection{1:2}
- :MEASure:HORizontal:DTIMe:ENUMber{1:2}
- :MEASure:HORizontal:DTIMe:ETHReshold{1:2}
- :MEASure:HORizontal:DTIMe:FAVorite
- :MEASure:HORizontal:DTIMe:LOCation?
- :MEASure:HORizontal:DTIMe:REGion
- :MEASure:HORizontal:DTIMe:SOURce
- :MEASure:HORizontal:DTIMe:STATus?
- :MEASure:HORizontal:DTIMe:STATus:DETails?
- :MEASure:HORizontal:DTIMe:STATus:REASon?
- :MEASure:HORizontal:DTIMe:UREFerence:STATe
- :MEASure:HORizontal:DTIMe:UREFerence:VALue

## Query Syntax

    :MEASure:HORizontal:DTIMe:STATus:DETails?

## Description

Returns a string that may provide additional details for a failed `:MEASure:HORizontal:DTIMe` measurement. If the measurement was successful, a null string is returned.

For a basic description of a measurement failure, use the `:MEASure:HORizontal:DTIMe:STATus:REASon?` sibling query. Use the `:MEASure:HORizontal:DTIMe:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors