# :MEASure:EYE:PAM:LINearity:STATus:DETails?

Eye Linearity Commands

- :MEASure:EYE:PAM:LINearity
- :MEASure:EYE:PAM:LINearity:DEFinition
- :MEASure:EYE:PAM:LINearity:FAVorite
- :MEASure:EYE:PAM:LINearity:LOCation?
- :MEASure:EYE:PAM:LINearity:SOURce
- :MEASure:EYE:PAM:LINearity:STATus?
- :MEASure:EYE:PAM:LINearity:STATus:DETails?
- :MEASure:EYE:PAM:LINearity:STATus:REASon?

## Query Syntax

    :MEASure:EYE:PAM:LINearity:STATus:DETails?

## Description

Returns a string that may provide additional details for a failed `:MEASure:EYE:PAM:LINearity` measurement. If the measurement was successful, a null string is returned.

For a basic description of a measurement failure, use the `:MEASure:EYE:PAM:LINearity:STATus:REASon?` sibling query. Use the `:MEASure:EYE:PAM:LINearity:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors