# :SOURce Simulated Commands

Simulated and AWG Commands

- :SOURce:AMPLitude
- :SOURce:CDIVide
- :SOURce:DIFFerential
- :SOURce:FILTer:CUToff
- :SOURce:FILTer:RTIMe
- :SOURce:FILTer:STATe
- :SOURce:FILTer:TYPE
- :SOURce:FNAMe
- :SOURce:FORMat
- :SOURce:FOTWo:JITTer
- :SOURce:FOTWo:STATe
- :SOURce:FUNCtion
- :SOURce:INVert
- :SOURce:JITTer:BLIMit
- :SOURce:JITTer:BLSTate
- :SOURce:JITTer:DRJ?
- :SOURce:JITTer:DRN?
- :SOURce:JITTer:RJ
- :SOURce:JITTer:STATe
- :SOURce:LEVel
- :SOURce:NOISe:RN
- :SOURce:NOISe:STATe
- :SOURce:OENable
- :SOURce:OFFSet
- :SOURce:PATTern
- :SOURce:PLENgth
- :SOURce:PWIDth
- :SOURce:SEED
- :SOURce:SKEW
- :SOURce:SRATe
- :SOURce:SSC:FREQuency
- :SOURce:SSC:PATTern
- :SOURce:SSC:PERCent
- :SOURce:SSC:PHASe
- :SOURce:SSC:PPM
- :SOURce:SSC:STATe
- :SOURce:SSC:STYPe
- :SOURce:WTYPe

To install a simulated instrument, use the `:INSTrument` subsystem's `:INSTrument:CONNection:SELection` command. Use the `:SOURce:WTYPe` command to select the type of source waveform, which could be data, clock, function, or file. After defining the waveform, use `:SOURce:OENable` command to enable the source output and the `:CHANnel:DISPlay` command to display the waveform.