# :MEASure:HORizontal:DCYCle:EDIRection

Duty Cycle Commands

- :MEASure:HORizontal:DCYCle
- :MEASure:HORizontal:DCYCle:EDIRection
- :MEASure:HORizontal:DCYCle:FAVorite
- :MEASure:HORizontal:DCYCle:LOCation?
- :MEASure:HORizontal:DCYCle:OCCurrences
- :MEASure:HORizontal:DCYCle:REGion
- :MEASure:HORizontal:DCYCle:SOURce
- :MEASure:HORizontal:DCYCle:STATus?
- :MEASure:HORizontal:DCYCle:STATus:DETails?
- :MEASure:HORizontal:DCYCle:STATus:REASon?
- :MEASure:HORizontal:DCYCle:UREFerence:STATe
- :MEASure:HORizontal:DCYCle:UREFerence:VALue

## Command Syntax

    :MEASure:HORizontal:DCYCle:EDIRection  {RISing | FALLing}

## Query Syntax

    :MEASure:HORizontal:DCYCle:EDIRection?

## Description

For the duty cycle measurement, specifies the edge on which to start the measurement.

- `RISing` — the cycle(s) on which the measurement is made begin with a rising edge.
- `FALLing` — the cycle(s) on which the measurement is made begin with a falling edge.