# :LTESt:MEASure:MLIMit:CFMargin

:LTESt Measurement Setup Commands

- :LTESt:MEASure:MLIMit:CFMargin
- :LTESt:MEASure:MLIMit:CFResults
- :LTESt:MEASure:MLIMit:FREGion
- :LTESt:MEASure:MLIMit:LLIMit
- :LTESt:MEASure:MLIMit:SOFailure
- :LTESt:MEASure:MLIMit:SOURce:LOCation
- :LTESt:MEASure:MLIMit:SOURce:TYPE
- :LTESt:MEASure:MLIMit:STATe
- :LTESt:MEASure:MLIMit:ULIMit
- :LTESt:MEASure:MLIMit:UPACtion

## Command Syntax

    :LTESt:MEASure:MLIMitN:CFMargin <pct_margin>

Where N identifies one of sixteen {1:16} limit tests.

<pct_margin> is a double.

## Query Syntax

    :LTESt:MEASure:MLIMitN:CFMargin?

## Description

When copying the lower and upper measurement limits from the current measurement results (see `:LTESt:MEASure:MLIMit:CFResults`), this command specifies the percent margin that is applied to the measurement results before being copied to the lower and upper limits.

If the % margin is set to 0%, the minimum and maximum values are copied exactly to the limits, increasing the likelihood of a failure.

Setting a % margin decreases the minimum limit and increases the maximum limit by the entered percentage of the measurement result Range (Max - Min).