# :MEASure:EYE:PAM:OVERshoot:STATus?

PAM Overshoot Commands

- :MEASure:EYE:PAM:OVERshoot
- :MEASure:EYE:PAM:OVERshoot:FAVorite
- :MEASure:EYE:PAM:OVERshoot:LOCation?
- :MEASure:EYE:PAM:OVERshoot:SOURce
- :MEASure:EYE:PAM:OVERshoot:STATus?
- :MEASure:EYE:PAM:OVERshoot:STATus:DETails?
- :MEASure:EYE:PAM:OVERshoot:STATus:REASon?
- :MEASure:EYE:PAM:OVERshoot:THRatio

## Query Syntax

    :MEASure:EYE:PAM:OVERshoot:STATus?

## Query Response

    {CORR | INV | QUES}

`CORR`
  The measurement result is correct.
`INV`
  The measurement result is invalid. A question mark (?) is shown in the displayed results table instead of a measurement result.
`QUES`
  The measurement result is questionable. A question mark (?) is shown in the displayed results table next to the measurement result.

## Description

Queries the status of the `:MEASure:EYE:PAM:OVERshoot` measurement. Use the `:MEASure:EYE:PAM:OVERshoot:STATus:REASon?` child query to determine the reason for a invalid or questionable measurement.

## See Also

- Measurement Errors