# :MEASure:VERTical:VTIMe:TIME

Amplitude-at-Time Commands

- :MEASure:VERTical:VTIMe
- :MEASure:VERTical:VTIMe:FAVorite
- :MEASure:VERTical:VTIMe:LOCation?
- :MEASure:VERTical:VTIMe:REGion
- :MEASure:VERTical:VTIMe:SOURce
- :MEASure:VERTical:VTIMe:STATus?
- :MEASure:VERTical:VTIMe:STATus:DETails?
- :MEASure:VERTical:VTIMe:STATus:REASon?
- :MEASure:VERTical:VTIMe:TIME
- :MEASure:VERTical:VTIMe:UREFerence:STATe
- :MEASure:VERTical:VTIMe:UREFerence:VALue

## Command Syntax

    :MEASure:VERTical:VTIMe:TIME<time>

<time> is a double.

## Query Syntax

    :MEASure:VERTical:VTIMe:TIME?

## Description

Specifies the time at which the Amplitude-at-Time measurement is made. Use the `:MEASure:VERTical:VTIMe` to make the measurement.

## Example Command Sequence

    :MEASure:VERTical:VTIMe:SOURce CHAN1_1
    :MEASure:VERTical:VTIMe:TIME 200E-12
    :MEASure:VERTical:VTIMe
    :MEASure:VERTical:VTIMe?