# :NETWorks:TRACe:DISPlay

:NETWorks:TRACe General Commands

- :NETWorks:TRACe:COLor
- :NETWorks:TRACe:CWINdow
- :NETWorks:TRACe:DISPlay
- :NETWorks:TRACe:NETWork
- :NETWorks:TRACe:OPERator
- :NETWorks:TRACe:PARameter
- :NETWorks:TRACe:STATus?
- :NETWorks:TRACe:UNAMe?

## Command Syntax

    :NETWorks:TRACeN:DISPlay {ON | OFF}

Where N identifies a specific trace and must be selected from 1 to 128 {1:128}.

## Query Syntax

    :NETWorks:TRACe{1:128}:DISPlay?

## Description

Turns the display of an S-parameter trace on or off.