# :MEASure:HORizontal:STIMe:STATus:DETails?

Setup Time Commands

- :MEASure:HORizontal:STIMe
- :MEASure:HORizontal:STIMe:CEDirection
- :MEASure:HORizontal:STIMe:DEDirection
- :MEASure:HORizontal:STIMe:FAVorite
- :MEASure:HORizontal:STIMe:LOCation?
- :MEASure:HORizontal:STIMe:OCCurrences
- :MEASure:HORizontal:STIMe:REGion
- :MEASure:HORizontal:STIMe:SOURce
- :MEASure:HORizontal:STIMe:STATus?
- :MEASure:HORizontal:STIMe:STATus:DETails?
- :MEASure:HORizontal:STIMe:STATus:REASon?
- :MEASure:HORizontal:STIMe:UREFerence:STATe
- :MEASure:HORizontal:STIMe:UREFerence:VALue

## Query Syntax

    :MEASure:HORizontal:STIMe:STATus:DETails?

## Description

Returns a string that may provide additional details for a failed `:MEASure:HORizontal:STIMe` measurement. If the measurement was successful, a null string is returned.

For a basic description of a measurement failure, use the `:MEASure:HORizontal:STIMe:STATus:REASon?` sibling query. Use the `:MEASure:HORizontal:STIMe:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors