# :MEASure:JITTer:JITTer:DIMensions

Jitter Setup Commands

- :MEASure:JITTer:BSCale
- :MEASure:JITTer:GSCale
- :MEASure:JITTer:JITTer:ANALysis
- :MEASure:JITTer:JITTer:DIMensions
- :MEASure:JITTer:JITTer:DMAXimized
- :MEASure:JITTer:JITTer:EDGE
- :MEASure:JITTer:JITTer:EOPening
- :MEASure:JITTer:JITTer:EOPening:PROBability
- :MEASure:JITTer:JITTer:FLAG
- :MEASure:JITTer:JITTer:FLEad
- :MEASure:JITTer:JITTer:MODE
- :MEASure:JITTer:JITTer:NUINtervals
- :MEASure:JITTer:JITTer:PTYPe
- :MEASure:JITTer:JITTer:RJBandwidth
- :MEASure:JITTer:JITTer:RJComp
- :MEASure:JITTer:JITTer:RJCResult?
- :MEASure:JITTer:JITTer:RJCValue
- :MEASure:JITTer:JITTer:RJSTabilize
- :MEASure:JITTer:JITTer:RJSValue
- :MEASure:JITTer:JITTer:SMEThod
- :MEASure:JITTer:JITTer:TJBer
- :MEASure:JITTer:JITTer:UNITs
- :MEASure:JITTer:SOURce

## Command Syntax

    :MEASure:JITTerN:JITTer:DIMensions  <left_col>,<right_col>

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

<left_col> and <right_col> are whole or decimal numbers.

## Query Syntax

    :MEASure:JITTerN:JITTer:DIMensions?

## Description

Specifies the proportions of the left-column statistics table and the right-column jitter graphs within the Jitter results window.

The width of a column is the number specified, divided by the sum of all the numbers specified, times the total display width. For example, to specify left and right column widths of 60% and 40%, respectively, you can use the dimensions of "0.6,0.4", "6,4", "60,40", etc.