# :DISK Documentation Wizard Commands

:DISK Doc Wizard Commands

- :DISK:DWIZard:DBHertz{1:4}:SDATa
- :DISK:DWIZard:DHERtz{1:4}:SDATa
- :DISK:DWIZard:DOUTput:SDATa
- :DISK:DWIZard:ECResults:SDATa
- :DISK:DWIZard:FNAMe
- :DISK:DWIZard:FPResults{1:64}:SDATa
- :DISK:DWIZard:HRESults{1:4}:SDATa
- :DISK:DWIZard:IRESponse{1:4}:SDATa
- :DISK:DWIZard:JITTer{1:4}:SDATa
- :DISK:DWIZard:LFMagnitude:SDATa
- :DISK:DWIZard:LLTResults:SDATa
- :DISK:DWIZard:MARKers:SDATa
- :DISK:DWIZard:MHIStogram{1:4}:SDATa
- :DISK:DWIZard:MTESt{1:16}:SDATa
- :DISK:DWIZard:NOISe{1:4}:SDATa
- :DISK:DWIZard:PNMWindow:SDATa
- :DISK:DWIZard:PROTocol{1:4}:SDATa
- :DISK:DWIZard:RESults:SDATa
- :DISK:DWIZard:SAVE
- :DISK:DWIZard:SHERtz{1:4}:SDATa
- :DISK:DWIZard:SRESponse{1:4}:SDATa
- :DISK:DWIZard:SSCReen
- :DISK:DWIZard:SSETup
- :DISK:DWIZard:SSINfo
- :DISK:DWIZard:SSParam
- :DISK:DWIZard:TIME{1:4}:SDATa
- :DISK:DWIZard:WAVE:H5Format

Configures and saves a Documentation Wizard file (.zip). Use the `:DISK:DWIZard:FNAMe` command to specify the name of saved file and the `:DISK:DWIZard:SAVE` command to actually save the file. To select the type of information that is saved in the zip file, use the commands shown in the following table. The files that get saved are listed in the command descriptions.

Commands Used to Select Data to Save
Item Selected with Command | Saved in Zip File
--- | ---
:DISK:DWIZard:DBHertz{1:4}:SDATa | Decibels (Hz) window data
:DISK:DWIZard:DHERtz{1:4}:SDATa | Degrees (Hz) window data
:DISK:DWIZard:ECResults:SDATa | Eye Contours results
:DISK:DWIZard:FPResults{1:64}:SDATa | FFT Peaks results
:DISK:DWIZard:HRESults{1:4}:SDATa | Waveform Histogram results
:DISK:DWIZard:IRESponse{1:4}:SDATa | Impulse Response plot
:DISK:DWIZard:JITTer{1:4}:SDATa | Jitter results window
:DISK:DWIZard:LFMagnitude:SDATa | Log-Freq-Mag plot from Phase Noise analysis
:DISK:DWIZard:LLTResults:SDATa | Limit Line Test results
:DISK:DWIZard:MARKers:SDATa | Markers results
:DISK:DWIZard:MHIStogram{1:4}:SDATa | Measurement Histogram results
:DISK:DWIZard:MTESt{1:16}:SDATa | Mask Test results
:DISK:DWIZard:NOISe{1:4}:SDATa | Noise results window
:DISK:DWIZard:PNMWindow:SDATa | Phase Noise Marker results
:DISK:DWIZard:PROTocol{1:4}:SDATa | Protocol listing window
:DISK:DWIZard:RESults:SDATa | Measurement results
:DISK:DWIZard:SHERtz{1:4}:SDATa | Seconds (Hz) window data
:DISK:DWIZard:SRESponse{1:4}:SDATa | Step Response plot
:DISK:DWIZard:SSCReen | Screen capture of entire display
:DISK:DWIZard:SSETup | Instrument setup file
:DISK:DWIZard:SSINfo | System information
:DISK:DWIZard:SSParam | S-Parameter files
:DISK:DWIZard:TIME{1:4}:SDATa | Waveform window data

## Example

    :DISK:DWIZard:SSCReen ON
    :DISK:DWIZard:SSETup ON
    :DISK:DWIZard:SSINfo OFF
    :DISK:DWIZard:RESults:SDATa ON
    :DISK:DWIZard:FNAMe "%USER_DATA_DIR%\Documentation Results\DocumentationResults_PAM4"
    :DISK:DWIZard:SAVE
    *OPC?