# :MEASure:EYE:CONTour:RJSTabilize

Eye Contour Configuration Commands

- Eye Contour Configuration Commands
- :MEASure:EYE:CONTour:BERates
- :MEASure:EYE:CONTour:DISPlay
- :MEASure:EYE:CONTour:PSPec
- :MEASure:EYE:CONTour:RJSTabilize
- :MEASure:EYE:CONTour:RJSValue:EYE
- :MEASure:EYE:CONTour:RNSTabilize
- :MEASure:EYE:CONTour:RNSValue:LEVel
- :MEASure:EYE:CONTour:SOURce

## Command Syntax

    :MEASure:EYE:CONTourN:RJSTabilize {ON | OFF}

Where N identifies a group of contour lines and must be {1:16}.

## Query Syntax

    :MEASure:EYE:CONTourN:RJSTabilize?

## Description

Turns on or off Random Jitter (RJ) stabilization for a group of eye-contour lines. When RJ stabilization is on, use the `:MEASure:EYE:CONTour:RJSValue:EYE` command to enter a separate value of RJ for each eye. To measure the RJ, measure the RJ while using a signal that has a short pattern. Or, measure the RJ using a separate instrument. Each eye-contour line group has its own RJ stabilization values.