# Amplitude Measurements

Measurements

- Time Measurements
- Amplitude Measurements
- Clock Measurements
- Data Measurements
- SNDR Measurements
- PAM Measurements
- FFT Measurements
- User-Defined Measurements
- NRZ Eye Measurements
- PAM Eye Measurements
- Mask Test Commands
- Querying Measurement Results and Statistics

These measurements are optimized for NRZ signals but, as noted, may work with PAM signals.

- :MEASure:VERTical:VAMPlitude (Amplitude)
- :MEASure:VERTical:VLOWer (Amplitude at Lower)
- :MEASure:VERTical:VMIDdle (Amplitude at Middle)
- :MEASure:VERTical:VUPPer (Amplitude at Upper)
- :MEASure:VERTical:VTIMe (Amplitude at Time)
- :MEASure:VERTical:VAVerage (Average)
- :MEASure:VERTical:CPOWer (Carrier Power)
- :MEASure:VERTical:CROSsing (Crossing)
- :MEASure:VERTical:OVERshoot (Overshoot)
- :MEASure:VERTical:PREShoot (Preshoot)
- :MEASure:VERTical:VMAXimum (Maximum)
- :MEASure:VERTical:VMINimum (Minimum)
- :MEASure:VERTical:VPP (Peak-Peak Amplitude)
- :MEASure:VERTical:PPHRatio (Peak-Peak at Hit Ratio)
- :MEASure:VERTical:VRMS (RMS)
- :MEASure:VERTical:VBASe (Waveform Base)
- :MEASure:VERTical:VTOP (Waveform Top)