# :WMEMory:EYE:UIXRange

:WMEMory EYE Commands

- :WMEMory EYE Commands
- :WMEMory:EYE:BITS
- :WMEMory:EYE:CCOunt
- :WMEMory:EYE:CURSor
- :WMEMory:EYE:CWINdow
- :WMEMory:EYE:DISPlay
- :WMEMory:EYE:PATTern
- :WMEMory:EYE:UIXPosition
- :WMEMory:EYE:UIXRange
- :WMEMory:EYE:UUNits
- :WMEMory:EYE:WINDow:COPY
- :WMEMory:EYE:WINDow:LEFT
- :WMEMory:EYE:WINDow:METHod
- :WMEMory:EYE:WINDow:RIGHt
- :WMEMory:EYE:WINDow:TRACking
- :WMEMory:EYE:WINDow:WIDTh
- :WMEMory:EYE:XPOSition
- :WMEMory:EYE:XSCale

## Command Syntax

    :WMEMoryN:EYE:UIXRange <time_in_UI>

Where N identifies one of eight {1:8} possible waveform memories. For example, `:WMEMory4`.

<time_in_UI> is a double in UI (unit interval) units.

## Query Syntax

    :WMEMoryN:EYE:UIXRange?

## Description

Sets the waveform memory N horizontal time range (width) of the real-time eye display in UI units.

This command directly affects the real-time eye's horizontal time/div setting in seconds (see the `:WMEMory:EYE:XSCale` command).

To set the horizontal position (center display location) of the real-time eye display in UI units, use the `:WMEMory:EYE:UIXPosition` command.

Only the center UI is valid for the recovered clock edge. You can display up to 10 UIs to show context before and after the center UI.