# :MEASure:VERTical:VRMS:AREA

Vrms Commands

- :MEASure:VERTical:VRMS
- :MEASure:VERTical:VRMS:AREA
- :MEASure:VERTical:VRMS:EDIRection
- :MEASure:VERTical:VRMS:FAVorite
- :MEASure:VERTical:VRMS:LOCation?
- :MEASure:VERTical:VRMS:REGion
- :MEASure:VERTical:VRMS:SOURce
- :MEASure:VERTical:VRMS:STATus?
- :MEASure:VERTical:VRMS:STATus:DETails?
- :MEASure:VERTical:VRMS:STATus:REASon?
- :MEASure:VERTical:VRMS:TYPE
- :MEASure:VERTical:VRMS:UREFerence:STATe
- :MEASure:VERTical:VRMS:UREFerence:VALue

## Command Syntax

    :MEASure:VERTical:VRMS:AREA  {CYCLe | REGion}

## Query Syntax

    :MEASure:VERTical:VRMS:AREA?

## Description

Configures the VRMS measurement (`:MEASure:VERTical:VRMS`) data to be sampled across the entire region (`:MEASure:VERTical:VRMS:REGion`) or a single cycle (`CYCle`).