# :LTESt:MEASure:SWAVeform:RESet

:LTESt Measurement Waveform Commands

- :LTESt:MEASure:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:MEASure:SWAVeform:CHANnel:FTYPe
- :LTESt:MEASure:SWAVeform:CHANnel{N}:STATe
- :LTESt:MEASure:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:MEASure:SWAVeform:CMODe{N}:FNAMe
- :LTESt:MEASure:SWAVeform:CMODe:FTYPe
- :LTESt:MEASure:SWAVeform:CMODe{N}:STATe
- :LTESt:MEASure:SWAVeform:CMODe{N}:WMEMory
- :LTESt:MEASure:SWAVeform:DIFF{N}:FNAMe
- :LTESt:MEASure:SWAVeform:DIFF:FTYPe
- :LTESt:MEASure:SWAVeform:DIFF{N}:STATe
- :LTESt:MEASure:SWAVeform:DIFF{N}:WMEMory
- :LTESt:MEASure:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:MEASure:SWAVeform:FUNCtion{N}:STATe
- :LTESt:MEASure:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:MEASure:SWAVeform:RESet

## Command Syntax

    :LTESt:MEASure:SWAVeform:RESet

## Description

For measurement limit testing, turns off the reporting action of saving waveforms. Reporting for all waveforms is disabled. There is no query form of this command.