# :MEASure:VERTical:PREShoot:EDIRection

Preshoot Commands

- :MEASure:VERTical:PREShoot
- :MEASure:VERTical:PREShoot:EDIRection
- :MEASure:VERTical:PREShoot:FAVorite
- :MEASure:VERTical:PREShoot:LOCation?
- :MEASure:VERTical:PREShoot:OCCurrences
- :MEASure:VERTical:PREShoot:REGion
- :MEASure:VERTical:PREShoot:SOURce
- :MEASure:VERTical:PREShoot:STATus?
- :MEASure:VERTical:PREShoot:STATus:DETails?
- :MEASure:VERTical:PREShoot:STATus:REASon?
- :MEASure:VERTical:PREShoot:UREFerence:STATe
- :MEASure:VERTical:PREShoot:UREFerence:VALue

## Command Syntax

    :MEASure:VERTical:PREShoot:EDIRection {RISing | FALLing}

## Query Syntax

    :MEASure:VERTical:PREShoot:EDIRection?

## Description

For the `:MEASure:VERTical:PREShoot` measurement, this command specifies which signal edges to include in the measurement.

## Example Command Sequence

    :MEASure:VERTical:PREShoot:SOURce CHAN1_1
    :MEASure:VERTical:PREShoot:EDIRection RISing
    :MEASure:VERTical:PREShoot
    :MEASure:VERTical:PREShoot?