# :MEASure:JITTer:JITTer:EWIDth:STATus:DETails?

Jitter Eye Width Commands

- :MEASure:JITTer:JITTer:EWIDth?
- :MEASure:JITTer:JITTer:EWIDth:STATus?
- :MEASure:JITTer:JITTer:EWIDth:STATus:DETails?
- :MEASure:JITTer:JITTer:EWIDth:STATus:REASon?

## Query Syntax

    :MEASure:JITTerN:JITTer:EWIDth:STATus:DETails?

Where N identifies one of four possible jitter/noise analyses {1:4}. For example, `JITTer4`.

## Description

Returns a string that may provide additional details for a failed `:MEASure:JITTer:JITTer:EWIDth?` measurement. If the measurement was successful, a null string is returned.

For a basic description of a measurement failure, use the `:MEASure:JITTer:JITTer:EWIDth:STATus:REASon?` sibling query. Use the `:MEASure:JITTer:JITTer:EWIDth:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors