# :MEASure:DATA:NOISe:STATus:REASon?

Noise Commands

- :MEASure:DATA:NOISe
- :MEASure:DATA:NOISe:FAVorite
- :MEASure:DATA:NOISe:LDETection
- :MEASure:DATA:NOISe:LEVel
- :MEASure:DATA:NOISe:LOCation?
- :MEASure:DATA:NOISe:MLOCation
- :MEASure:DATA:NOISe:OCCurrences
- :MEASure:DATA:NOISe:SOURce
- :MEASure:DATA:NOISe:STATus?
- :MEASure:DATA:NOISe:STATus:DETails?
- :MEASure:DATA:NOISe:STATus:REASon?
- :MEASure:DATA:NOISe:UNITs
- :MEASure:DATA:NOISe:UREFerence:STATe
- :MEASure:DATA:NOISe:UREFerence:VALue

## Query Syntax

    :MEASure:DATA:NOISe:STATus:REASon?

## Query Response

Refer to the table "Common Reasons for INV or QUES Status".

## Description

Returns a string that explains the reason for a failed `:MEASure:DATA:NOISe` measurement. If the measurement was successful, a null string is returned.

Additional information about the failure may be available using the `:MEASure:DATA:NOISe:STATus:DETails?` sibling query. Use the `:MEASure:DATA:NOISe:STATus?` parent query to determine if the measurement has failed.

## See Also

- Measurement Errors