# :WAVeform:STATus?

:WAVeform General Commands

- :WAVeform:CLIPped?
- :WAVeform:HOLes?
- :WAVeform:SOURce
- :WAVeform:STATus?
- :WAVeform:STATus:DETails?
- :WAVeform:STATus:REASon?

## Query Syntax

    :WAVeform:STATus?

## Description

Queries the status of the waveform data and returns the strings shown in the following table. Use the `:WAVeform:STATus:REASon?` child query to return a string that indicates why the data is invalid or questionable.

STATus? Query Response
Response | Description
--- | ---
CORR | The waveform data is correct.
INV | The waveform data is invalid.
QUES | The waveform data is questionable.

Query the data using one of the following commands:

- :WAVeform:YFORmat:ASCii:YDATa?
- :WAVeform:YFORmat:DOUBle:YDATa?
- :WAVeform:YFORmat:FLOat:YDATa?
- :WAVeform:YFORmat:WORD:YDATa?
- :WAVeform:XYFormat:ASCii:YDATa?
- :WAVeform:XYFormat:ASCii:XDATa?
- :WAVeform:XYFormat:DOUBle:YDATa?
- :WAVeform:XYFormat:DOUBle:XDATa?
- :WAVeform:XYFormat:FLOat:YDATa?
- :WAVeform:XYFormat:FLOat:XDATa?

## Child Commands

- `:WAVeform:STATus:DETails?`
- `:WAVeform:STATus:REASon?`