# :NETWorks:DFILe:PTYPe?

:NETWorks:DFILe Commands

- :NETWorks:DFILe Commands
- :NETWorks:DFILe:CLEar
- :NETWorks:DFILe:DSTatus?
- :NETWorks:DFILe:DSTatus:REASon?
- :NETWorks:DFILe:ENABle?
- :NETWorks:DFILe:FILE:LOAD
- :NETWorks:DFILe:FILE:NAME
- :NETWorks:DFILe:PTYPe?

## Query Syntax

    :NETWorks:DFILe{1:4}:PTYPe?

## Description

Queries the selected memory to determine the type of S-parameters that it holds. The possible return values are listed in the following table.

Query Response Versus Data in Memory
Query Response | Number of DUT Ports | Number of S-Parameters | Source File Type
--- | --- | --- | ---
Single-Ended DUTs
SPOR1 | 1 | 1 | .s1p, or .txt
Differential DUTs
DPOR1 | 1 | 4 | .s2p
DPOR2 | 2 | 16 | .s4p
DPOR4 | 4 | 64 | .s8p
DPOR6 | 6 | 144 | .s12p
DPOR8 | 8 | 256 | .s16p