# :CALibrate:CALibrator:PWIDth

:CALibrate Calibrator Commands

- :CALibrate:CALibrator:AOENable
- :CALibrate:CALibrator:DCOFfset
- :CALibrate:CALibrator:ESPeed
- :CALibrate:CALibrator:MODE
- :CALibrate:CALibrator:PWIDth
- :CALibrate:CALibrator:SPULse

## Command Syntax

    :CALibrate:CALibrator:PWIDth  <time>

<time> is a double.

## Query Syntax

    :CALibrate:CALibrator:PWIDth?

## Description

When the Pulse Positive, Pulse Positive Single, Pulse Negative, or Pulse Negative Single calibrator mode is selected (see `:CALibrate:CALibrator:MODE`), this command specifies the width of the pulse.