# :DISPlay:WINDow:DHERtz{N}:LOCation

:DISPlay Freq Domain Windows Commands

- :DISPlay:WINDow:DBHertz{N}:DMODe
- :DISPlay:WINDow:DBHertz{N}:LEGend:EXPand
- :DISPlay:WINDow:DBHertz{N}:LOCation
- :DISPlay:WINDow:DBHertz{N}:TOPMost
- :DISPlay:WINDow:DBHertz{N}:TSIGnal
- :DISPlay:WINDow:DHERtz{N}:DMODe
- :DISPlay:WINDow:DHERtz{N}:LEGend:EXPand
- :DISPlay:WINDow:DHERtz{N}:LOCation
- :DISPlay:WINDow:DHERtz{N}:TOPMost
- :DISPlay:WINDow:DHERtz{N}:TSIGnal
- :DISPlay:WINDow:SHERtz{N}:DMODe
- :DISPlay:WINDow:SHERtz{N}:LEGend:EXPand
- :DISPlay:WINDow:SHERtz{N}:LOCation
- :DISPlay:WINDow:SHERtz{N}:TOPMost
- :DISPlay:WINDow:SHERtz{N}:TSIGnal

## Command Syntax

    :DISPlay:WINDow:DHERtzN:LOCation {A1 | A2 | A3 | A4
       | B1 | B2 | B3 | B4
       | C1 | C2 | C3 | C4
       | D1 | D2 | D3 | D4 | FLOat | MAXimize | MINimize}

Where N indicates one of 4 possible Degrees (Hz) windows. For example, `DHERtz2`.

## Query Syntax

    :DISPlay:WINDow:DHERtzN:LOCation?

## Query Response

    {A1 | A2 | A3 | A4
       | B1 | B2 | B3 | B4
       | C1 | C2 | C3 | C4
       | D1 | D2 | D3 | D4 | FLO | MAX | MIN}

## Description

Selects the location to display a Degrees (Hz) waveform content window. Use the arguments listed below to specify the position.

Display Panel Locations
A1 | A2 | A3 | A4
B1 | B2 | B3 | B4
C1 | C2 | C3 | C4
D1 | D2 | D3 | D4

FLOat
  The content window is undocked (floated) from Infiniium's window. To re-dock the window, resend the command using the `A1`, `A2`, `A3`, `A4`, `B1`, `B2`, `B3`, `B4`, `C1`, `C2`, `C3`, `C4`, `D1`, `D2`, `D3`, or `D4` arguments.
MAXimize
  The content window occupies the space of all nine panel locations.
MINimize
  The content window is lowered to a task bar.

## Example Command Sequence

    :DISPlay:WINDow:DHERtz2:LOCation C3

## Sibling Commands

- `:DISPlay:WINDow:DHERtz{N}:DMODe`
- `:DISPlay:WINDow:DHERtz{N}:LEGend:EXPand`
- `:DISPlay:WINDow:DHERtz{N}:TOPMost`