# :LTESt:ACQuire:SWAVeform:CHANnel{N}:WMEMory

:LTESt Acquisition Commands

- :LTESt:ACQuire:CTYPe
- :LTESt:ACQuire:CTYPe:SAMPles
- :LTESt:ACQuire:CTYPe:WAVeforms
- :LTESt:ACQuire:SIMage:FNAMe
- :LTESt:ACQuire:SIMage:FNAMe:AUPDate
- :LTESt:ACQuire:SIMage:FNAMe:USTandard
- :LTESt:ACQuire:SIMage:FTYPe?
- :LTESt:ACQuire:SIMage:IMETadata
- :LTESt:ACQuire:SIMage:INVert
- :LTESt:ACQuire:SIMage:MONochrome
- :LTESt:ACQuire:SIMage:SINClude
- :LTESt:ACQuire:SIMage:STATe
- :LTESt:ACQuire:SIMage:WINDow
- :LTESt:ACQuire:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CHANnel:FTYPe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:STATe
- :LTESt:ACQuire:SWAVeform:CHANnel{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:CMODe{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:CMODe:FTYPe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:STATe
- :LTESt:ACQuire:SWAVeform:CMODe{N}:WMEMory WMEMory{1:8}
- :LTESt:ACQuire:SWAVeform:DIFF{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:DIFF:FTYPe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:STATe
- :LTESt:ACQuire:SWAVeform:DIFF{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:FNAMe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:STATe
- :LTESt:ACQuire:SWAVeform:FUNCtion{N}:WMEMory
- :LTESt:ACQuire:SWAVeform:RESet

## Command Syntax

    :LTESt:ACQuire:SWAVeform:CHANnel{N}:WMEMory WMEMory{1:8}

CHANnel{N} identifies the channel as in CHANnel1_1, CHANnel1_2, …, CHANnel8_8.

## Query Syntax

    :LTESt:ACQuire:SWAVeform:CHANnel{N}:WMEMory?

## Description

Upon completion of an acquisition limit test, selects a waveform memory as a destination to save a channel waveform. Use the `:LTESt:ACQuire:SWAVeform:CHANnel{N}:STATe` command to enable and disable waveform reporting for the channel. To enable or disable acquisition limit tests, use the `:LTESt:ACQuire:STATe` command.