# :MEASure:VERTical:OVERshoot:EDIRection

Overshoot Commands

- :MEASure:VERTical:OVERshoot
- :MEASure:VERTical:OVERshoot:EDIRection
- :MEASure:VERTical:OVERshoot:FAVorite
- :MEASure:VERTical:OVERshoot:LOCation?
- :MEASure:VERTical:OVERshoot:OCCurrences
- :MEASure:VERTical:OVERshoot:REGion
- :MEASure:VERTical:OVERshoot:SOURce
- :MEASure:VERTical:OVERshoot:STATus?
- :MEASure:VERTical:OVERshoot:STATus:DETails?
- :MEASure:VERTical:OVERshoot:STATus:REASon?
- :MEASure:VERTical:OVERshoot:UREFerence:STATe
- :MEASure:VERTical:OVERshoot:UREFerence:VALue

## Command Syntax

    :MEASure:VERTical:OVERshoot:EDIRection {RISing | FALLing}

## Query Syntax

    :MEASure:VERTical:OVERshoot:EDIRection?

## Description

For the `:MEASure:VERTical:OVERshoot` measurement, this command specifies which signal edges to include in the measurement.

## Example Command Sequence

    :MEASure:VERTical:OVERshoot:SOURce CHAN1_1
    :MEASure:VERTical:OVERshoot:EDIRection RISing
    :MEASure:VERTical:OVERshoot
    :MEASure:VERTical:OVERshoot?