# :MEASure:VERTical:VRMS:EDIRection

Vrms Commands

- :MEASure:VERTical:VRMS
- :MEASure:VERTical:VRMS:AREA
- :MEASure:VERTical:VRMS:EDIRection
- :MEASure:VERTical:VRMS:FAVorite
- :MEASure:VERTical:VRMS:LOCation?
- :MEASure:VERTical:VRMS:REGion
- :MEASure:VERTical:VRMS:SOURce
- :MEASure:VERTical:VRMS:STATus?
- :MEASure:VERTical:VRMS:STATus:DETails?
- :MEASure:VERTical:VRMS:STATus:REASon?
- :MEASure:VERTical:VRMS:TYPE
- :MEASure:VERTical:VRMS:UREFerence:STATe
- :MEASure:VERTical:VRMS:UREFerence:VALue

## Command Syntax

    :MEASure:VERTical:VRMS:EDIRection  {RISing | FALLing}

## Query Syntax

    :MEASure:VERTical:VRMS:EDIRection?

## Description

For the VRMS measurement, when the selected area is a single cycle:

- `RISing` or `FALLing` — the cycle beginning with this edge that is nearest to the timebase reference is the cycle to measure.