# Factory Default

Click Setup > Factory Default to restore Infiniium to its factory default settings.

Factory Default resets all settings including general, trigger, probe, channel skew, preferences, and instrument connection settings.

A Default Setup resets only general and trigger settings. See Default Setup.

User preference and instrument connection settings after a Factory Default are listed in the following tables.

Preference Settings
Feature | See
--- | ---
Notification selections | Infiniium Display Overview
Open setup file include settings | Open Setup Files
Badge height and wrap | Analog Channels Setup
Waveform color settings | Waveform Color
External Scaling | External Scaling
Multi-Purpose button settings | Multi-Purpose Button
Favorite measurements | Add Measurements Dialog Box
Vertical Divisions | Display Setup (Graticule tab)
UI Theme | Display Setup (Appearance tab)
Invert Signal Display Windows
Spectrum Colors
Dialog Opacity
Dialog Size
Use On-Screen Keyboard
Dock Message Area
Show Timebase Status Button
Full-Screen Zoomed Mode
SCPI Recorder playback speed | SCPI Recorder
SCPI Server Setup | SCPI Server Setup
SCPI byte order | Programmer's Guide

Instrument Connection Settings
Feature | Setting after Factory Default (on PC)
--- | ---
Connection 1 | Virtual Real-Time Scope
Channel 1 Simulation Source | On Data Source: NRZ, PRBS-7, 9.95328 Gbd, 500 mV amplitude, 0 V offset Filter: 4th order Bessel, 15 GHz bandwidth Jitter & Noise: 100 fs random jitter, 2 mV random noise
Acquisition Run Mode | On