# :SYSTem:MODel?

Information Commands

- :SYSTem:DATE?
- :SYSTem:EMBedded?
- :SYSTem:HELP:HEADers?
- :SYSTem:HREVision?
- :SYSTem:MODel?
- :SYSTem:OPTions?
- :SYSTem:OSYStem?
- :SYSTem:PERSona:MANufacturer
- :SYSTem:PERSona:MANufacturer:DEFault
- :SYSTem:PERSona:MODel
- :SYSTem:PERSona:MODel:DEFault
- :SYSTem:SERial?
- :SYSTem:SIGNal:TYPE?
- :SYSTem:TEMPerature?
- :SYSTem:TEMPerature:STABle?
- :SYSTem:TIME?
- :SYSTem:UTCNow?

## Query Syntax

    :SYSTem:MODel? [{FRAMe | CONNection{1:8}}]

## Description

Returns the model number of Infiniium oscilloscope. An example of a returned string is XR804KA or D9300A when offline.

FRAMe
  When Infiniium is connected to an oscilloscope, the returned string will be something like `XR804KA`. When Infiniium is not connected to an instrument, the returned string will be `D9300A`. `FRAMe` is the default argument if no argument is provided.
CONNection{1:8}

  For the specified connection number, returns the model number of the connected instrument. If a simulated instrument is assigned to a connection, the string "D9300A" is returned and, in this case, you can use the `:INSTrument:CONNection:SELection` query to determine the type of simulated instrument.

  The string "Not Present" is returned if an instrument is not installed at the connection. For a multi-connection instrument, specify the left most connection. For example, for an instrument installed at connections 3 and 4, specify `CONNection3`.